D – Yes . as You can see , by dividing the whole processing into little parts , we would take less hardware because we can reuse the hardware for multiple times and by dividing it and then concating the results at the end , we may decrease the amount of frequency of the clock which increases the speed of calcualtion ( it seems like you are simulating a multi-threading system on a hardware )